My global print settings in Cura

3D-Printer:		Creality CR10 mini (DriektDrive) 

Quality:
layer height		0,15 mm
layer width		0,38 mm
first layer height		105%

Casing:
number of wall lines		     4
upper layers		     4
lower layers		     4
only smooth the top layer	yes
alternating additional walls	yes

Infill:
filling			100%

Material:
fliament			PLA (3d Jake)
nozzle			0,4 mm
hotend heat: 		210°
bed heat			 50°
(all) flow			100%

Speed:
print speed		50 mm/s
fill speed			50 mm/s
wall speed			25 mm/s

Movements:
Feeding			5 mm
Combing modus		not in the outer skin
Cooling			yes (default)

Support:
support			yes / all over

Printing plate adhesion:	individually

Note: Holes have to be reworked to get a perfect fit

		TL_all_easy



 


